
# Version 13.0.0
Standard allPIXAneo NXGE
## Component Versions
|      Variant      |         Version         |
|   ------------    |      -------------      |
| Bitstream         |          30.2.0         |
| Application/XML   |          21.1.0         |
| Bootfile          |          25.1.0         |
| Feature Reference |          21.1.0         |
| Gamma    	        |      KaxGamma03_10      |


## Notes




## Changes and new Features

* Internal refactoring regarding the LED-Flashing.
* Minimum **GainControlRegionOffsetY** and **GainControlRegionHeight** is now 1.
* Log mainboard temperature every 5'C temperature change.
* More temporary freedom in configuring the **MasterSlaveSource**/**MasterSlaveOutput** features.
  * The validity will be checked before **AcquisitionStart** or during **AcquisitionArm**
* Checking the **LedFlashSequenceTime** parameter depends on the LineStart trigger now.
* Added NoCache for **MasterSlaveSourceReg** node for feature update when selecting Default.
* Support BPC component


## Bug Fixes

* Fixed bugs related to LED-Flashing
* Fixed the bug of led flash control in speed2high case
* Fixed Bugs regarding loading the **Gamma**
* Fixed sensor shut down during over heat. (issue for some hardware)
* Fixed the bug in checking line time when led flashing is active.
* Fixed the bug in updating the **MasterSlaveSource** user set entry. (Update from old user set less than 13.0.0)
  * Related to internal line.
* Fixed the bug in setting **MasterSlaveOutput** to off.
* Fixed bugs related to gain control region.
* Fixed the bug for **BinningHorizontal** when used with **ImageCalibrationLineDistance**. (Related to DVAL relaxation)


## Incompatibilities

* LED-Flashing
	* In order to fix LED-Flashing issues the minimum **LedFlashSequenceTime** has been increased by 0.5us.
	* This refers also to the minimum value during the triggered mode.
* **ImageStreamWidthReg** feature will not return 0 anymore if no region is enabled, but the sensor width. 


## Errata


* Using LED-Flash and MasterSlave mode together will not work for the slave camera.
  * Independently the features are working.
* When using **MasterSlaveMode** and **FrameActive** the incoming frame active signal must not exceed the configured height in the **Height** feature.
  * Otherwise issues on the slave camera will occur.


## Docs

