
# Version 8.0.0
Standard allPIXAneo NXGE
## Component Versions
|      Variant      |         Version         |
|   ------------    |      -------------      |
| Bitstream         |          27.2.0         |
| Application/XML   |          15.2.3         |
| Bootfile          |          21.0.0         |
| Feature Reference |          15.2.3         |
| Gamma    	        |      KaxGamma03_10      |


## Notes

* From package 6.0.0 only the enabled LED-Flash outputs are configured.
  * From package 6.0.0 the outputs may be floating. Consider this if you have them connected somewhere.
  * In former packages the unused LED-Flash outputs still were driven by the camera.


## Changes and new Features

* Changed the vendor name, default model name and manufacturer info for Allied Vision
* Line features are not locked anymore by Trigger Features
* The DeviceStatusCode can recover from errors
* Support AcquisitionArm feature
* Line time and exposure time can be set independent of each other limits. (Not in GCT)
  * Further it can be checked either by AcquisitionArm feature or during acquisition start
* Internal refactoring
  * I2C clock frequency
  * Register addresses (Applications 15.0.0 require at least bitstream 26.0.0)
* Modified enabling of some internal image processing components. (Set transparent values instead of switching off the component)
* Renamed the sensor training done status code
* New sensor configuration to extend the reset level range.


## Bug Fixes

* Fixed the bug in the deprecated DSNU/PRNU data set information features.
* Fixed the bug of missing last pixels when generating the internal DSNU/PRNU reference. (Mono cameras only)


## Incompatibilities


* New sensor configuration.
  * New DSNU/PRNU references are suggested


## Errata


* Limitations for mono mode:
  * The Gain Control Region value may not be precisely located
  * The Gain Control Region current values, may not be precise
* Led flash may not work properly
  * With some settings camera does not deliver any images
  * With some other settings there can be one pattern missing


## Docs

* Marked unused device specific error codes
* Marked LUT_CTRL_ERR error category removed
* Added AcquisitionArm feature