
# Version 9.0.0
Standard allPIXAneo NXGE
## Component Versions
|      Variant      |         Version         |
|   ------------    |      -------------      |
| Bitstream         |          27.4.0         |
| Application/XML   |          16.1.1         |
| Bootfile          |          21.0.0         |
| Feature Reference |          16.1.1         |
| Gamma    	        |      KaxGamma03_10      |


## Notes




## Changes and new Features

* Removed support for binning value 16
* Relaxing the throughput depending on the required line time. (DVAL)
  * For some use cases (GigE) this may help to reduce package loss.
* Improved the acquisition test to detect errors.
* Support color transformation 12bit co-efficients


## Bug Fixes

* Modifications regarding internal scan cancel register usage to avoid issues. (Region configuration and Trigger Mode on to off)
* Bug fix of pin stripe test pattern in 4-Channel mode.
* p6 mono
	* Fixed the bug in internal DSNU/PRNU reference capturing for the last pixels


## Incompatibilities

* Binning value 16 is not supported


## Errata


* Limitations for mono mode:
  * The Gain Control Region value may not be precisely located
  * The Gain Control Region current values, may not be precise
* Led flash may not work properly
  * With some settings camera does not deliver any images
  * With some other settings there can be one pattern missing


## Docs

* Updated binning value range 